NCITE Intersection Traffic Control Committee Meeting Minutes
February 17, 2021 – 8:00 to 10:00 a.m.
Virtual Microsoft Teams Meeting
I. Introductions
· Chair: Cade Botten cade.botten@hennepin.us 
· Co-chair: Ben Brasser benjamin.brasser@minneapolis.gov 
· Members Present – Cade Botten, Ben Brasser, Daniel Truhler, Marty Carlson, Quanzakari DeChiara-Crillion, Kao Sua Yang, Steve Rippey, Jerry Kotzenmacher, Joel Hinnenkamp, Daniel Hogan, Mike Fairbanks, John Fahrendorf, Roger Plum, Kevin Chan, Phil Kulis, Joe Gustafson, Kevin Schwartz, Ryan Anderson, Don Van Gorp, Nick Erpelding, Jeremy Melquist, Tom Fidler, Mike Klobucar, Tyler Krage, Sue Zarling, Mark Callahan

II. Discussion of Proposed Amendments to MUTCD
· FYA using 3-section Head
· Reaction is generally uncertain that this is a beneficial treatment
· Potential for operational confusion
· Limited cost savings to retrofit signals due to wiring, labor needs

· Signal Installation for Speed Control
· Understand the idea behind the guidance
· Unsure if the word “penalize” is going to be understood in correct context

· Separating Signal Faces w/ Different Movements
· Consistent with expectations and previous requirements; 3-foot spacing is relatively generous

· Separate Turn Signal Face Requires Exclusive Turn Lane
· Agree with guidance

· Max Yellow Times
· Some uncertainty regarding 6-second maximum yellow, particularly on high-speed approaches
· This guidance relates to the new ITE Recommended Practice: suggestion to revisit the ITE recommended practice at a later meeting

· Omit Peds ONLY During RR Preemption
· Agree with this guidance; consistent with current practice and MnMUTCD

· Transitioning Out of Yellow-Red Flash
· No disagreement with yellow-red flash guidance as proposed
· Would like to see improved/updated guidance for exiting from red-red flash

· Pedestrian Intervals
· Measuring ped clearance times from edge of pavement is consistent with existing practice
· Noteworthy change to requirements for minimum Walk interval where Leading Pedestrian Interval is used and no Accessible Pedestrian Signal is present: may result in the need to lengthen Walk time in the controller

· Pedestrian Pushbutton Locator Tones
· Agree with added flexibility

· Prohibition of Flashing Confirmation EVP Light
· Prohibiting the flashing EVP confirmation light is contrary to current practice 
· Agencies consider this to be a significant issue and plan to raise comments

· Interim Approvals Included in Proposed Amendments
· Bike signal and RRFB interim approvals are relatively unchanged in how they’re included in proposed MUTCD amendments

III. Round Robin
· Cade B mentioned meeting invite challenges using the mailing list. Future meeting invites will be sent two ways to ensure delivery to everyone. Members should contact Cade if they did not receive an invite to this meeting.
· [bookmark: _GoBack]Ben B mentioned that bike signals and RRFBs are included in proposed amendments; relatively unchanged from their Interim Approval and Official Interpretation language
· Jeremy M raised the question of the timeline for maintaining/removing “Left Turn Yield on FYA” signs. Others shared responses that their agencies are either leaving them indefinitely or removing them after 6 months. MnDOT guidance is to remove if there is an opportunity any time following 6 months of operation; several locations remain in place for much longer.
· Jerry K mentioned the MnDOT Signals 101 class will be held online in March and encouraged anyone to reach out to him if interested
· Ken L asked City of Minneapolis for any updates regarding feedback/operations related to bike signals along Washington Ave. Ben B stated signal operations have not changed recently and will look into any comments to follow up 
